| Hard Disk Sentinel www.hdsentinel.com

# Physical Disk Information - Disk: #1: ST9160821AS

### Hard Disk Summary

| Hard Disk Number | : | 1
| Interface | : | SAT Standard USB/ATA
| Vendor Information | : | VID: 152D, PID: 2338
| Hard Disk Model ID | : | ST9160821AS
| Firmware Revision | : | 3.ALC
| Hard Disk Serial Number | : | 5MACC3H0
| Total Size | : | 152625 MB
| Power State | : | Active
| Current Temperature | : | 22 °C
| Maximum Temperature (Ever Measured) | : | 22 °C, 7.2.2012 ã. 20:29:22
| Minimum Temperature (Ever Measured) | : | 22 °C, 7.2.2012 ã. 20:29:22
| Maximum Temperature (During Entire Lifespan) | : | 61 °C
| Power On Time | : | 123 days, 21 hours
| Estimated Remaining Lifetime | : | more than 1000 days

| Health | : |

100 % (Excellent)
| Performance | : |

100 % (Excellent)

The hard disk status is PERFECT. Problematic or weak sectors were not found and there are no spin up or data transfer errors. No actions needed.

### ATA Information

| Hard Disk Cylinders | : | 310101
| Hard Disk Heads | : | 16
| Hard Disk Sectors | : | 63
| ATA Revision | : | ATA/ATAPI-7
| Total Sectors | : | 312581808
| Bytes Per Sector | : | 512
| Buffer Size | : | 8192 KB
| Multiple Sectors | : | 16
| Error Correction Bytes | : | 4
| Unformatted Capacity | : | 152628 MB
| Maximum PIO Mode | : | 4
| Maximum Multiword DMA Mode | : | 2
| Maximum UDMA Mode | : | 150 MB/s (6)
| Active UDMA Mode | : | 150 MB/s (6)
| Minimum Multiword DMA Transfer Time | : | 120 ns
| Recommended Multiword DMA Transfer Time | : | 120 ns
| Minimum PIO Transfer Time Without IORDY | : | 240 ns
| Minimum PIO Transfer Time With IORDY | : | 120 ns
| ATA Control Byte | : | Valid
| ATA Checksum Value | : | Valid

### Acoustic Management Configuration

| Acoustic Management | : | Not supported
| Acoustic Management | : | Disabled
| Current Acoustic Level | : | Default (00h)
| Recommended Acoustic Level | : | Max performance and volume (FEh)

### ATA Features

| Read Ahead Buffer | : | Supported, Enabled
| DMA | : | Supported
| Ultra DMA | : | Supported
| S.M.A.R.T. | : | Supported
| Power Management | : | Supported
| Write Cache | : | Supported
| Host Protected Area | : | Supported
| Advanced Power Management | : | Supported, Enabled
| Advanced Power Management Level | : | Minimum power consumption without standby (128)
| Extended Power Management | : | Not supported
| Power Up In Standby | : | Not supported
| 48-Bit LBA Addressing | : | Supported
| Device Configuration Overlay | : | Supported
| IORDY Support | : | Supported
| Read/Write DMA Queue | : | Not supported
| NOP Command | : | Not supported
| Trusted Computing | : | Not supported
| 64-Bit World Wide ID | : | Not supported
| Streaming | : | Not supported
| Media Card Pass Through | : | Not supported
| General Purpose Logging | : | Not supported
| Error Logging | : | Supported
| CFA Feature Set | : | Not supported
| CFast Device | : | Not supported
| Long Physical Sectors (1) | : | Not supported
| Long Logical Sectors | : | Not supported
| Write-Read-Verify | : | Supported, Disabled
| NV Cache Feature | : | Not supported
| NV Cache Power Mode | : | Not supported
| NV Cache Size | : | Not supported
| Free-fall Control | : | Not supported
| Free-fall Control Sensitivity | : | Not supported

### SSD Features

| Data Set Management | : | Not supported
| TRIM Command | : | Not supported
| Deterministic Read After TRIM | : | Not supported

### S.M.A.R.T. Details

| Off-line Data Collection Status | : | Successfully Completed
| Self Test Execution Status | : | Successfully Completed
| Total Time To Complete Off-line Data Collection | : | 426 seconds
| Execute Off-line Immediate | : | Supported
| Abort/restart Off-line By Host | : | Not supported
| Off-line Read Scanning | : | Supported
| Short Self-test | : | Supported
| Extended Self-test | : | Supported
| Conveyance Self-test | : | Not supported
| Selective Self-Test | : | Supported
| Save Data Before/After Power Saving Mode | : | Supported
| Enable/Disable Attribute Autosave | : | Supported
| Error Logging Capability | : | Supported
| Short Self-test Estimated Time | : | 1 minutes
| Extended Self-test Estimated Time | : | 111 minutes
| Last Short Self-test Result | : | Never Started
| Last Short Self-test Date | : | Never Started
| Last Extended Self-test Result | : | Never Started
| Last Extended Self-test Date | : | Never Started

### Security Mode

| Security Mode | : | Supported
| Security Erase | : | Not supported
| Security Erase Time | : | Not supported
| Security Enhanced Erase Feature | : | Not supported
| Security Enhanced Erase Time | : | Not supported
| Security Enabled | : | No
| Security Locked | : | No
| Security Frozen | : | No
| Security Counter Expired | : | No
| Security Level | : | High

### Serial ATA Features

| S-ATA Compliance | : | Yes
| S-ATA I Signaling Speed (1.5 Gps) | : | Supported
| S-ATA II Signaling Speed (3 Gps) | : | Not supported
| S-ATA Gen3 Signaling Speed (6 Gps) | : | Not supported
| Receipt Of Power Management Requests From Host | : | Not supported
| PHY Event Counters | : | Supported
| Non-Zero Buffer Offsets In DMA Setup FIS | : | Not supported
| DMA Setup Auto-Activate Optimization | : | Not supported
| Device Initiating Interface Power Management | : | Supported, Disabled
| In-Order Data Delivery | : | Not supported
| Asynchronous Notification | : | Not supported
| Software Settings Preservation | : | Supported, Enabled
| Native Command Queuing (NCQ) | : | Supported
| Queue Length | : | 32

### Disk Information

| Disk Family | : | Momentus 5400.3 160821
| Form Factor | : | 2.5"
| Capacity | : | 160 GB (160 x 1 000 000 000 bytes)
| Number Of Disks | : | 2
| Number Of Heads | : | 4
| Rotational Speed | : | 5400 RPM
| Rotation Time | : | 11,11 ms
| Average Rotational Latency | : | 5,56 ms
| Disk Interface | : | Serial-ATA/150
| Buffer-Host Max. Rate | : | 150 MB/seconds
| Buffer Size | : | 8192 KB
| Drive Ready Time (Typical) | : | ? seconds
| Average Seek Time | : | 12,5 ms
| Track To Track Seek Time | : | ? ms
| Full Stroke Seek Time | : | ? ms
| Width | : | 69,9 mm (2,8 inch)
| Depth | : | 100,2 mm (3,9 inch)
| Height | : | 9,5 mm (0,4 inch)
| Weight | : | 102 grams (0,2 pounds)
| Acoustic (Idle) | : | 2,3 Bel
| Acoustic (Min Performance And Volume) | : | 2,5 Bel
| Acoustic (Max Performance And Volume) | : | 3,0 Bel
| Required Power For Spinup | : | 1 200 mA
| Power Required (Seek) | : | 2,4 W
| Power Required (Idle) | : | 1,2 W
| Power Required (Standby) | : | 0,4 W
| Manufacturer | : | Seagate Technology
| Manufacturer Website | : | http://www.seagate.com/www/en-us/products

### S.M.A.R.T.

| No. | Attribute | Threshold | Value | Worst | Data | Status | Flags
| 1 | Raw Read Error Rate | 6 | 117 | 95 | 0000073B8E98 | OK | Error-Rate, Performance, Statistical, Critical
| 3 | Spin Up Time | 0 | 99 | 99 | 000000000000 | OK (Always passing) | Statistical, Critical
| 4 | Start/Stop Count | 20 | 97 | 97 | 000000000CD5 | OK | Self Preserving, Event Count, Statistical
| 5 | Reallocated Sectors Count | 36 | 100 | 100 | 000000000000 | OK | Self Preserving, Event Count, Statistical, Critical
| 7 | Seek Error Rate | 30 | 72 | 60 | 000505F1CAD2 | OK | Error-Rate, Performance, Statistical, Critical
| 9 | Power On Time Count | 0 | 97 | 97 | 000000000B9D | OK (Always passing) | Self Preserving, Event Count, Statistical
| 10 | Spin Retry Count | 34 | 100 | 100 | 000000000000 | OK | Event Count, Statistical, Critical
| 12 | Drive Power Cycle Count | 20 | 97 | 97 | 000000000D45 | OK | Self Preserving, Event Count, Statistical
| 187 | Reported Uncorrectable Errors | 0 | 100 | 100 | 000000000000 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 189 | High Fly Writes | 0 | 98 | 98 | 000000000002 | OK (Always passing) | Self Preserving, Event Count, Error-Rate, Statistical
| 190 | Airflow Temperature | 45 | 78 | 39 | 000016160016 | OK | Self Preserving, Statistical
| 192 | Power off Retract Cycle Count | 0 | 99 | 99 | 000000000878 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 193 | Load/Unload Cycle Count | 0 | 57 | 57 | 00000001519F | OK (Always passing) | Self Preserving, Event Count, Statistical
| 194 | Disk Temperature | 0 | 22 | 61 | 000E00000016 | OK (Always passing) | Self Preserving, Statistical
| 195 | Hardware ECC Recovered | 0 | 104 | 60 | 00000DDA3AD2 | OK (Always passing) | Event Count, Error-Rate, Statistical
| 197 | Current Pending Sector Count | 0 | 100 | 100 | 000000000000 | OK (Always passing) | Event Count, Statistical
| 198 | Off-Line Uncorrectable Sector Count | 0 | 100 | 100 | 000000000000 | OK (Always passing) | Event Count
| 199 | Ultra ATA CRC Error Count | 0 | 200 | 200 | 000000000000 | OK (Always passing) | Self Preserving, Event Count, Error-Rate, Performance, Statistical
| 200 | Write Error Rate | 0 | 100 | 253 | 000000000000 | OK (Always passing) |
| 202 | Data Address Mark Errors | 0 | 100 | 253 | 000000000000 | OK (Always passing) | Self Preserving, Event Count, Statistical

### Transfer Rate Information

| Total Data Read | : | 91 MB, 91 MB since installation (15.12.2011 ã.)
| Total Data Write | : | 90 MB, 90 MB since installation
| Average Reads Per Day | : | 1,69 MB
| Average Writes Per Day | : | 1,67 MB
| Current Transfer Rate | : | 0 KB/s
| Maximum Transfer Rate | : | 45 KB/s
| Current Read Rate | : | 0 KB/s
| Current Write Rate | : | 0 KB/s
| Current Disk Activity | : | 0 %