| Hard Disk Sentinel www.hdsentinel.com

# Physical Disk Information - Disk: #1: ST9500325AS

### Hard Disk Summary

| Hard Disk Number | : | 1
| Interface | : | SAT Standard USB/ATA
| Vendor Information | : | VID: 152D, PID: 2338
| Hard Disk Model ID | : | ST9500325AS
| Firmware Revision | : | 0002SDM1
| Hard Disk Serial Number | : | 5VE58HYR
| Total Size | : | 476937 MB
| Power State | : | Active
| Current Temperature | : | 21 °C
| Maximum Temperature (Ever Measured) | : | 26 °C, 7.2.2012 ã. 18:20:19
| Minimum Temperature (Ever Measured) | : | 17 °C, 7.2.2012 ã. 13:24:00
| Maximum Temperature (During Entire Lifespan) | : | 49 °C
| Power On Time | : | 460 days, 5 hours
| Estimated Remaining Lifetime | : | more than 1000 days

| Health | : |

97 % (Excellent)
| Performance | : |

100 % (Excellent)

There are 3 bad sectors on the disk surface. The contents of these sectors were moved to the spare area. At this point, warranty replacement of the disk is not yet possible, only if the health drops further. It is recommended to examine the log of the disk regularly. All new problems found will be logged there.
No actions needed.

### ATA Information

| Hard Disk Cylinders | : | 969021
| Hard Disk Heads | : | 16
| Hard Disk Sectors | : | 63
| ATA Revision | : | ATA8-ACS version 4
| Transport Version | : | SATA Rev 2.6
| Total Sectors | : | 976773168
| Bytes Per Sector | : | 512
| Buffer Size | : | 8192 KB
| Multiple Sectors | : | 16
| Error Correction Bytes | : | 4
| Unformatted Capacity | : | 476940 MB
| Maximum PIO Mode | : | 4
| Maximum Multiword DMA Mode | : | 2
| Maximum UDMA Mode | : | 300 MB/s (6)
| Active UDMA Mode | : | 300 MB/s (6)
| Minimum Multiword DMA Transfer Time | : | 120 ns
| Recommended Multiword DMA Transfer Time | : | 120 ns
| Minimum PIO Transfer Time Without IORDY | : | 120 ns
| Minimum PIO Transfer Time With IORDY | : | 120 ns
| ATA Control Byte | : | Valid
| ATA Checksum Value | : | Valid

### Acoustic Management Configuration

| Acoustic Management | : | Not supported
| Acoustic Management | : | Disabled
| Current Acoustic Level | : | Default (00h)
| Recommended Acoustic Level | : | Max performance and volume (FEh)

### ATA Features

| Read Ahead Buffer | : | Supported, Enabled
| DMA | : | Supported
| Ultra DMA | : | Supported
| S.M.A.R.T. | : | Supported
| Power Management | : | Supported
| Write Cache | : | Supported
| Host Protected Area | : | Supported
| Advanced Power Management | : | Supported, Enabled
| Advanced Power Management Level | : | Minimum power consumption without standby (128)
| Extended Power Management | : | Not supported
| Power Up In Standby | : | Not supported
| 48-Bit LBA Addressing | : | Supported
| Device Configuration Overlay | : | Supported
| IORDY Support | : | Supported
| Read/Write DMA Queue | : | Not supported
| NOP Command | : | Not supported
| Trusted Computing | : | Not supported
| 64-Bit World Wide ID | : | 005000C5F21BCEF1
| Streaming | : | Not supported
| Media Card Pass Through | : | Not supported
| General Purpose Logging | : | Supported
| Error Logging | : | Supported
| CFA Feature Set | : | Not supported
| CFast Device | : | Not supported
| Long Physical Sectors (1) | : | Not supported
| Long Logical Sectors | : | Not supported
| Write-Read-Verify | : | Supported, Disabled
| NV Cache Feature | : | Not supported
| NV Cache Power Mode | : | Not supported
| NV Cache Size | : | Not supported
| Free-fall Control | : | Not supported
| Free-fall Control Sensitivity | : | Not supported
| Nominal Media Rotation Rate | : | 5400 RPM

### SSD Features

| Data Set Management | : | Not supported
| TRIM Command | : | Not supported
| Deterministic Read After TRIM | : | Not supported

### S.M.A.R.T. Details

| Off-line Data Collection Status | : | Never Started
| Self Test Execution Status | : | Successfully Completed
| Total Time To Complete Off-line Data Collection | : | 0 seconds
| Execute Off-line Immediate | : | Supported
| Abort/restart Off-line By Host | : | Not supported
| Off-line Read Scanning | : | Not supported
| Short Self-test | : | Supported
| Extended Self-test | : | Supported
| Conveyance Self-test | : | Supported
| Selective Self-Test | : | Supported
| Save Data Before/After Power Saving Mode | : | Supported
| Enable/Disable Attribute Autosave | : | Supported
| Error Logging Capability | : | Supported
| Short Self-test Estimated Time | : | 1 minutes
| Extended Self-test Estimated Time | : | 139 minutes
| Conveyance Self-test Estimated Time | : | 2 minutes
| Last Short Self-test Result | : | Successfully Completed
| Last Short Self-test Date | : | 7.2.2012 ã. 13:32:51
| Last Short Self-test Duration | : | 1 minutes
| Last Extended Self-test Result | : | Never Started
| Last Extended Self-test Date | : | Never Started
| Last Conveyance Self-test Result | : | Never Started
| Last Conveyance Self-test Date | : | Never Started

### Security Mode

| Security Mode | : | Supported
| Security Erase | : | Supported
| Security Erase Time | : | 66 minutes
| Security Enhanced Erase Feature | : | Supported
| Security Enhanced Erase Time | : | 66 minutes
| Security Enabled | : | No
| Security Locked | : | No
| Security Frozen | : | No
| Security Counter Expired | : | No
| Security Level | : | High

### Serial ATA Features

| S-ATA Compliance | : | Yes
| S-ATA I Signaling Speed (1.5 Gps) | : | Supported
| S-ATA II Signaling Speed (3 Gps) | : | Supported
| S-ATA Gen3 Signaling Speed (6 Gps) | : | Not supported
| Receipt Of Power Management Requests From Host | : | Not supported
| PHY Event Counters | : | Supported
| Non-Zero Buffer Offsets In DMA Setup FIS | : | Not supported
| DMA Setup Auto-Activate Optimization | : | Not supported
| Device Initiating Interface Power Management | : | Supported, Disabled
| In-Order Data Delivery | : | Not supported
| Asynchronous Notification | : | Not supported
| Software Settings Preservation | : | Supported, Enabled
| Native Command Queuing (NCQ) | : | Supported
| Queue Length | : | 32

### Disk Information

| Disk Family | : | Momentus 5400.6 500325
| Form Factor | : | 2.5"
| Capacity | : | 500 GB (500 x 1 000 000 000 bytes)
| Number Of Disks | : | 2
| Number Of Heads | : | 4
| Rotational Speed | : | 5400 RPM
| Rotation Time | : | 11,11 ms
| Average Rotational Latency | : | 5,56 ms
| Disk Interface | : | Serial-ATA/300
| Buffer-Host Max. Rate | : | 300 MB/seconds
| Buffer Size | : | 8192 KB
| Drive Ready Time (Typical) | : | ? seconds
| Average Seek Time | : | ? ms
| Track To Track Seek Time | : | ? ms
| Full Stroke Seek Time | : | ? ms
| Width | : | 69,9 mm (2,8 inch)
| Depth | : | 100,5 mm (4,0 inch)
| Height | : | 9,5 mm (0,4 inch)
| Weight | : | 98.8 grams (0,2 pounds)
| Acoustic (Idle) | : | 2,3 Bel
| Acoustic (Min Performance And Volume) | : | 2,5 Bel
| Acoustic (Max Performance And Volume) | : | 3,0 Bel
| Required Power For Spinup | : | 1 200 mA
| Power Required (Seek) | : | 2,4 W
| Power Required (Idle) | : | 1,2 W
| Power Required (Standby) | : | 0,4 W
| Manufacturer | : | Seagate Technology
| Manufacturer Website | : | http://www.seagate.com/www/en-us/products

### S.M.A.R.T.

| No. | Attribute | Threshold | Value | Worst | Data | Status | Flags
| 1 | Raw Read Error Rate | 6 | 118 | 99 | 00000B0921E8 | OK | Error-Rate, Performance, Statistical, Critical
| 3 | Spin Up Time | 0 | 98 | 98 | 000000000000 | OK (Always passing) | Statistical, Critical
| 4 | Start/Stop Count | 20 | 99 | 99 | 00000000074E | OK | Self Preserving, Event Count, Statistical
| 5 | Reallocated Sectors Count | 36 | 100 | 100 | 000000000003 | OK | Self Preserving, Event Count, Statistical, Critical
| 7 | Seek Error Rate | 30 | 81 | 60 | 00000780AC6F | OK | Error-Rate, Performance, Statistical, Critical
| 9 | Power On Time Count | 0 | 88 | 88 | 000000002B25 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 10 | Spin Retry Count | 97 | 100 | 100 | 000000000000 | OK | Event Count, Statistical, Critical
| 12 | Drive Power Cycle Count | 20 | 99 | 37 | 0000000006DD | OK | Self Preserving, Event Count, Statistical
| 184 | End-to-End Error Count | 99 | 100 | 100 | 000000000000 | OK | Self Preserving, Event Count, Statistical
| 187 | Reported Uncorrectable Errors | 0 | 63 | 63 | 000000000025 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 188 | Command Timeout | 0 | 100 | 98 | 000100010179 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 189 | High Fly Writes | 0 | 100 | 100 | 000000000000 | OK (Always passing) | Self Preserving, Event Count, Error-Rate, Statistical
| 190 | Airflow Temperature | 45 | 79 | 51 | 000016150015 | OK | Self Preserving, Statistical
| 191 | G-Sense Error Rate | 0 | 100 | 100 | 0000000000B4 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 192 | Power off Retract Cycle Count | 0 | 100 | 100 | 0000000000C0 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 193 | Load/Unload Cycle Count | 0 | 24 | 24 | 000000025499 | OK (Always passing) | Self Preserving, Event Count, Statistical
| 194 | Disk Temperature | 0 | 21 | 49 | 000800000015 | OK (Always passing) | Self Preserving, Statistical
| 195 | Hardware ECC Recovered | 0 | 48 | 42 | 00000B0921E8 | OK (Always passing) | Event Count, Error-Rate, Statistical
| 197 | Current Pending Sector Count | 0 | 100 | 100 | 000000000000 | OK (Always passing) | Event Count, Statistical
| 198 | Off-Line Uncorrectable Sector Count | 0 | 100 | 100 | 000000000000 | OK (Always passing) | Event Count
| 199 | Ultra ATA CRC Error Count | 0 | 200 | 200 | 000000000000 | OK (Always passing) | Self Preserving, Event Count, Error-Rate, Performance, Statistical
| 254 | Free Fall Event Count | 0 | 100 | 100 | 000000000000 | OK (Always passing) | Self Preserving, Event Count, Statistical

### Transfer Rate Information

| Total Data Read | : | 15 MB, 6 052 MB since installation (15.12.2011 ã.)
| Total Data Write | : | 0 MB, 0 MB since installation
| Average Reads Per Day | : | 112,07 MB
| Average Writes Per Day | : | 0,00 MB
| Current Transfer Rate | : | 0 KB/s
| Maximum Transfer Rate | : | 1 KB/s
| Current Read Rate | : | 0 KB/s
| Current Write Rate | : | 0 KB/s
| Current Disk Activity | : | 0 %